**PRICING FORM**

**Pembroke Canal Sheetpiling**

Note: all blank fields are to be filled in by the Contractor and all sheets form part of the BID

**December 2024**

# PRICING FORM

**PEMBROKE CANAL SHEETPILING**

NOTE: All work detailed on the contract documents shall be covered completely by the Grand Total. Individual lump sum items and rates are all-inclusive. If a specific task is not identified separately in the above list, the Contractor shall assume that it is included as part of another related listed item or items, or shall include it separately, and shall include it in the Grand Total amount. Overheads and margins are required for all labour and materials for the proposed works.

LUMP SUM BID

**TO: PERMANENT SECRETARY, Ministry of Public Works**

Having examined the bid documents for the above work, we the undersigned, offer to construct and complete the whole of the said works for the sum of:

(figures) BD$\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(words) BD$\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

We agree to abide by this bid for **thirty (30) calendar days** from the date fixed for receipt of bids, and understand that you may accept or reject any bid you may receive. We undertake to commence the works within fourteen calendar days of award of the Contract, and to complete the works by (date): .

We confirm having completed all parts of this form; and received and complied with all addenda (if any) as follows: Addenda #

**Signed:**

Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Block letters: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**On Behalf Of:**

Company name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Date:** \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Price Schedule

(To Be Completed By The Contractor)

All prices (in Bermuda dollars) are to be all inclusive of all other associated works as shown on the Contract Documents, materials, related accessories, storage, transport, assembly, placement, overhead and profit. These rates may be used for determining additions and deletions from the contract sum and for interim payment valuation.

| **ITEM** | **DESCRIPTION** | **LUMP SUM** |
| --- | --- | --- |
|  | **Mobilization** | | |
| 1.1 | Equipment rental |  |
| 1.2 | Establishment of temporary facilities |  |
| 1.3 | Establishment of working site boundaries including fencing, temporary pedestrian pathways etc. |  |
| 1.4 | Other items (please list below) |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **Sheetpiling** | | |
| 2.1 | Sheetpiling material costs |  |
| 2.2 | Prepare site and clear vegetation in preparation of sheetpiling. |  |
| 2.3 | Drive steel sheetpiles to meet dimensions and specifications as detailed in attached drawings. |  |
| 2.4 | Other items (please list below) |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **Cavity Cleaning and Pipe Penetrations** | | |
| 3.1 | Clean cavity between sheetpiling and existing masonry wall |  |
| 3.2 | Install pipe penetrations as per details in drawings |  |
| 3.3 | Other items (please list below) |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **Concrete Works** |  |
| 4.1 | Construct any formwork or shoring work as necessary |  |
| 4.2 | Pour concrete in space between sheet piling and existing wall |  |
| 4.3 | Install reinforcement and form capping beam |  |
| 4.4 | Other items (please list below) |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **Demobilization and Site Clean-up** | | |
| 5.1 | Remove and dispose of waste |  | |
| 5.2 | Demobilize equipment and facilities |  | |
| 5.3 | Site clean-up |  | |
| 5.4 | Other items (please list below) |  | |
|  |  |  |
|  |  |  |
|  |  |  |
|  | **Any items not listed above.** | | |
| 6.1 |  |  |
| 6.2 |  |  |
| 6.3 |  |  |
| 6.4 |  |  |
|  | **TOTAL** |  |

SCHEDULE OF UNIT RATES

(to be completed by the contractor)

All prices (in Bermuda dollars) in the schedule are to be **inclusive of materials and related accessories, storage, transport, plant and equipment assembly, placement, access, overhead and profit.** These rates may be used for determining additions to, and deletions from, the contract sum.

**ITEM UNIT RATE**

1. **Labour** 
   1. Unskilled Labour Hr $\_\_\_\_\_\_\_\_\_\_\_
   2. Skilled Labour Hr $\_\_\_\_\_\_\_\_\_\_\_
   3. Supervisor Hr $\_\_\_\_\_\_\_\_\_\_\_
   4. Welder Hr $\_\_\_\_\_\_\_\_\_\_\_
   5. Project Manager Hr $\_\_\_\_\_\_\_\_\_\_\_
2. **Equipment**
   1. Crane Day $\_\_\_\_\_\_\_\_\_\_
   2. Generator Day $\_\_\_\_\_\_\_\_\_\_
   3. Other Equipment not listed above. Please list below:

Hr / Day $\_\_\_\_\_\_\_\_\_\_

Hr / Day $\_\_\_\_\_\_\_\_\_\_

Hr / Day $\_\_\_\_\_\_\_\_\_\_

1. **Other Items not listed above**
   1. Steel Sheet Piling 20ft length section $\_\_\_\_\_\_\_\_\_\_\_
   2. Vegetation management yd3 $\_\_\_\_\_\_\_\_\_\_\_
   3. Supply/install concrete yd3 $\_\_\_\_\_\_\_\_\_\_\_
   4. Supply and install 10mm galv rebar LF $\_\_\_\_\_\_\_\_\_\_\_
   5. Supply and install 12mm galv rebar LF $\_\_\_\_\_\_\_\_\_\_\_

All unit rates above shall be considered fully inclusive of delivery, preparation, placing and finishing.

For variations to the contract not covered in the preceding price break down rates or the above schedule of unit rates, the price may be determined on the basis of the base material and installation cost plus  **%** for overhead and  **%** for profit and applied separately to the base cost.